Warnings from Oct 30, 2015 – Energy Puppy

To use system you must follow steps

1.Check for right polarity – phase connect to live and phase of load.

Line which carries power mark it – go to power supply find live and connect live to live.

2. Once connected sys to power supply leave for 2-3 days maybe to settle and nano coat – add small led light - 6 or 9-volt batteries to charge

3. Do not connect immediately ANY resistive loads like heaters, old light bulbs, do not use fan heater 2kw, ovens

4. Add 2nd small load – increase DC for about a week – 10 days

5) Small resistive load – 500 w - builds up over a week.

6) Build up from 2 to 5 kw

Cascade unit – additional unit in series – furthest point in house.

Then non-resistive is free

2nd unit feeding house – first unit

Put meters on 4 kw out 1 kw

Wind bars correctly – anti-clockwise

Nanocoating – use caustic for 2nd time be sure to get a homogeneous coating

Gans above copper above - always oxidation

Capacitors winding of paper or cloth is tight wind it anti clockwise

Do not dry gans on cloth or paper. Allow paste to dry

Center sun system – good amount of gans – not liquid but a paste

Always – bend your wires in at the ends – anti clockwise

When you turn wires need to touch when you turn them back – NO

Connect plasma to make - how you connect them – a stacker of 4 5 capacitors

Capacitor connections - anti-clockwise twists

Cascade capacitor (insulated material) – space between capacitors

Connect plates: neg to pos pos to neg

DO NOT worry about how the system will perform

Heating is only problem – toasters – heaters – DO NOT connect ANY chargers till after 3 weeks

Careful! Hand Drill – cutting system – 1000 rev power works produces 1500 rev

Car units: when you connect stacker unit - G line (-) M on top (+)

Bottom stacker (-) connected to manifold

Top stacker (+) connects to 1 capacitor (-)

Connect neg (-) of capacitor pos (+) to top stacker

Pos (+) of capacitor to battery (-)

Plasma unit next to fuel tank

Learn and teach about how to cut and use the plasma energy.

DO NOT CONNECT YOUR HOUSE UNIT TO YOUR CAR!

DO NOT USE YOUR CAR UNIT ON YOUR HOUSE!

Car unit: your AC is after connect to battery 1)DC and 1)AC is what’s used

House unit: connect to 50 hertz add stacker get entry

Do not use with tungsten lights, resistive loads